AVR Libc Home Page |  | AVR Libc Development Pages
Main Page | User Manual | Library Reference | FAQ | Alphabetical Index | Example Projects

# boot.h File Reference

## Defines
#define | _AVR_BOOT_H_ 1
#define | BOOTLOADER_SECTION __attribute__ ((section (".bootloader")))
#define | __COMMON_ASB RWWSB
#define | __COMMON_ASRE RWWSRE
#define | BLB12 5
#define | BLB11 4
#define | BLB02 3
#define | BLB01 2
#define | boot_spm_interrupt_enable() (__SPM_REG |= (uint8_t)_BV(SPMIE))
#define | boot_spm_interrupt_disable() (__SPM_REG &= (uint8_t)~_BV(SPMIE))
#define | boot_is_spm_interrupt() (__SPM_REG & (uint8_t)_BV(SPMIE))
#define | boot_rww_busy() (__SPM_REG & (uint8_t)_BV(__COMMON_ASB))
#define | boot_spm_busy() (__SPM_REG & (uint8_t)_BV(__SPM_ENABLE))
#define | boot_spm_busy_wait() do{}while(boot_spm_busy())
#define | __BOOT_PAGE_ERASE (_BV(__SPM_ENABLE) | _BV(PGERS))
#define | __BOOT_PAGE_WRITE (_BV(__SPM_ENABLE) | _BV(PGWRT))
#define | __BOOT_PAGE_FILL _BV(__SPM_ENABLE)
#define | __BOOT_RWW_ENABLE (_BV(__SPM_ENABLE) | _BV(__COMMON_ASRE))
#define | __BOOT_LOCK_BITS_SET (_BV(__SPM_ENABLE) | _BV(BLBSET))
#define | __boot_page_fill_normal(address, data)
#define | __boot_page_fill_alternate(address, data)
#define | __boot_page_fill_extended(address, data)
#define | __boot_page_erase_normal(address)
#define | __boot_page_erase_alternate(address)
#define | __boot_page_erase_extended(address)
#define | __boot_page_write_normal(address)
#define | __boot_page_write_alternate(address)
#define | __boot_page_write_extended(address)
#define | __boot_rww_enable()
#define | __boot_rww_enable_alternate()
#define | __boot_lock_bits_set(lock_bits)
#define | __boot_lock_bits_set_alternate(lock_bits)
#define | GET_LOW_FUSE_BITS (0x0000)
#define | GET_LOCK_BITS (0x0001)
#define | GET_EXTENDED_FUSE_BITS (0x0002)
#define | GET_HIGH_FUSE_BITS (0x0003)
#define | boot_lock_fuse_bits_get(address)
#define | __BOOT_SIGROW_READ (_BV(__SPM_ENABLE) | _BV(SIGRD))
#define | boot_signature_byte_get(addr)
#define | boot_page_fill(address, data) __boot_page_fill_normal(address, data)
#define | boot_page_erase(address) __boot_page_erase_normal(address)
#define | boot_page_write(address) __boot_page_write_normal(address)
#define | boot_rww_enable() __boot_rww_enable()
#define | boot_lock_bits_set(lock_bits) __boot_lock_bits_set(lock_bits)
#define | boot_page_fill_safe(address, data)
#define | boot_page_erase_safe(address)
#define | boot_page_write_safe(address)
#define | boot_rww_enable_safe()
#define | boot_lock_bits_set_safe(lock_bits)

## Detailed Description

## Define Documentation

#define __boot_lock_bits_set | ( | lock_bits |  | ) |

Value:

    (__extension__({                                           \
        uint8_t value = (uint8_t)(~(lock_bits));               \
        __asm__ __volatile__                                   \
        (                                                      \
            "ldi r30, 1\n\t"                                   \
            "ldi r31, 0\n\t"                                   \
            "mov r0, %2\n\t"                                   \
            "sts %0, %1\n\t"                                   \
            "spm\n\t"                                          \
            :                                                  \
            : "i" (_SFR_MEM_ADDR(__SPM_REG)),                  \
              "r" ((uint8_t)__BOOT_LOCK_BITS_SET),             \
              "r" (value)                                      \
            : "r0", "r30", "r31"                               \
        );                                                     \
    }))

#define __boot_lock_bits_set_alternate | ( | lock_bits |  | ) |

Value:

    (__extension__({                                           \
        uint8_t value = (uint8_t)(~(lock_bits));               \
        __asm__ __volatile__                                   \
        (                                                      \
            "ldi r30, 1\n\t"                                   \
            "ldi r31, 0\n\t"                                   \
            "mov r0, %2\n\t"                                   \
            "sts %0, %1\n\t"                                   \
            "spm\n\t"                                          \
            ".word 0xffff\n\t"                                 \
            "nop\n\t"                                          \
            :                                                  \
            : "i" (_SFR_MEM_ADDR(__SPM_REG)),                  \
              "r" ((uint8_t)__BOOT_LOCK_BITS_SET),             \
              "r" (value)                                      \
            : "r0", "r30", "r31"                               \
        );                                                     \
    }))

#define __boot_page_erase_alternate | ( | address |  | ) |

Value:

    (__extension__({                                 \
        __asm__ __volatile__                         \
        (                                            \
            "sts %0, %1\n\t"                         \
            "spm\n\t"                                \
            ".word 0xffff\n\t"                       \
            "nop\n\t"                                \
            :                                        \
            : "i" (_SFR_MEM_ADDR(__SPM_REG)),        \
              "r" ((uint8_t)__BOOT_PAGE_ERASE),      \
              "z" ((uint16_t)address)                \
        );                                           \
    }))

#define __boot_page_erase_extended | ( | address |  | ) |

Value:

    (__extension__({                                 \
        __asm__ __volatile__                         \
        (                                            \
            "movw r30, %A3\n\t"                      \
            "sts  %1, %C3\n\t"                       \
            "sts %0, %2\n\t"                         \
            "spm\n\t"                                \
            :                                        \
            : "i" (_SFR_MEM_ADDR(__SPM_REG)),        \
              "i" (_SFR_MEM_ADDR(RAMPZ)),            \
              "r" ((uint8_t)__BOOT_PAGE_ERASE),      \
              "r" ((uint32_t)address)                \
            : "r30", "r31"                           \
        );                                           \
    }))

#define __boot_page_erase_normal | ( | address |  | ) |

Value:

    (__extension__({                                 \
        __asm__ __volatile__                         \
        (                                            \
            "sts %0, %1\n\t"                         \
            "spm\n\t"                                \
            :                                        \
            : "i" (_SFR_MEM_ADDR(__SPM_REG)),        \
              "r" ((uint8_t)__BOOT_PAGE_ERASE),      \
              "z" ((uint16_t)address)                \
        );                                           \
    }))

#define __boot_page_fill_alternate | ( | address,
|  | data |  | ) |

Value:

    (__extension__({                                 \
        __asm__ __volatile__                         \
        (                                            \
            "movw  r0, %3\n\t"                       \
            "sts %0, %1\n\t"                         \
            "spm\n\t"                                \
            ".word 0xffff\n\t"                       \
            "nop\n\t"                                \
            "clr  r1\n\t"                            \
            :                                        \
            : "i" (_SFR_MEM_ADDR(__SPM_REG)),        \
              "r" ((uint8_t)__BOOT_PAGE_FILL),       \
              "z" ((uint16_t)address),               \
              "r" ((uint16_t)data)                   \
            : "r0"                                   \
        );                                           \
    }))

#define __boot_page_fill_extended | ( | address,
|  | data |  | ) |

Value:

    (__extension__({                                 \
        __asm__ __volatile__                         \
        (                                            \
            "movw  r0, %4\n\t"                       \
            "movw r30, %A3\n\t"                      \
            "sts %1, %C3\n\t"                        \
            "sts %0, %2\n\t"                         \
            "spm\n\t"                                \
            "clr  r1\n\t"                            \
            :                                        \
            : "i" (_SFR_MEM_ADDR(__SPM_REG)),        \
              "i" (_SFR_MEM_ADDR(RAMPZ)),            \
              "r" ((uint8_t)__BOOT_PAGE_FILL),       \
              "r" ((uint32_t)address),               \
              "r" ((uint16_t)data)                   \
            : "r0", "r30", "r31"                     \
        );                                           \
    }))

#define __boot_page_fill_normal | ( | address,
|  | data |  | ) |

Value:

    (__extension__({                                 \
        __asm__ __volatile__                         \
        (                                            \
            "movw  r0, %3\n\t"                       \
            "sts %0, %1\n\t"                         \
            "spm\n\t"                                \
            "clr  r1\n\t"                            \
            :                                        \
            : "i" (_SFR_MEM_ADDR(__SPM_REG)),        \
              "r" ((uint8_t)__BOOT_PAGE_FILL),       \
              "z" ((uint16_t)address),               \
              "r" ((uint16_t)data)                   \
            : "r0"                                   \
        );                                           \
    }))

#define __boot_page_write_alternate | ( | address |  | ) |

Value:

    (__extension__({                                 \
        __asm__ __volatile__                         \
        (                                            \
            "sts %0, %1\n\t"                         \
            "spm\n\t"                                \
            ".word 0xffff\n\t"                       \
            "nop\n\t"                                \
            :                                        \
            : "i" (_SFR_MEM_ADDR(__SPM_REG)),        \
              "r" ((uint8_t)__BOOT_PAGE_WRITE),      \
              "z" ((uint16_t)address)                \
        );                                           \
    }))

#define __boot_page_write_extended | ( | address |  | ) |

Value:

    (__extension__({                                 \
        __asm__ __volatile__                         \
        (                                            \
            "movw r30, %A3\n\t"                      \
            "sts %1, %C3\n\t"                        \
            "sts %0, %2\n\t"                         \
            "spm\n\t"                                \
            :                                        \
            : "i" (_SFR_MEM_ADDR(__SPM_REG)),        \
              "i" (_SFR_MEM_ADDR(RAMPZ)),            \
              "r" ((uint8_t)__BOOT_PAGE_WRITE),      \
              "r" ((uint32_t)address)                \
            : "r30", "r31"                           \
        );                                           \
    }))

#define __boot_page_write_normal | ( | address |  | ) |

Value:

    (__extension__({                                 \
        __asm__ __volatile__                         \
        (                                            \
            "sts %0, %1\n\t"                         \
            "spm\n\t"                                \
            :                                        \
            : "i" (_SFR_MEM_ADDR(__SPM_REG)),        \
              "r" ((uint8_t)__BOOT_PAGE_WRITE),      \
              "z" ((uint16_t)address)                \
        );                                           \
    }))

#define __boot_rww_enable | ( |  | ) |

Value:

    (__extension__({                                 \
        __asm__ __volatile__                         \
        (                                            \
            "sts %0, %1\n\t"                         \
            "spm\n\t"                                \
            :                                        \
            : "i" (_SFR_MEM_ADDR(__SPM_REG)),        \
              "r" ((uint8_t)__BOOT_RWW_ENABLE)       \
        );                                           \
    }))

#define __boot_rww_enable_alternate | ( |  | ) |

Value:

    (__extension__({                                 \
        __asm__ __volatile__                         \
        (                                            \
            "sts %0, %1\n\t"                         \
            "spm\n\t"                                \
            ".word 0xffff\n\t"                       \
            "nop\n\t"                                \
            :                                        \
            : "i" (_SFR_MEM_ADDR(__SPM_REG)),        \
              "r" ((uint8_t)__BOOT_RWW_ENABLE)       \
        );                                           \
    }))

Automatically generated by Doxygen 1.5.7 on 6 Nov 2008.